LEED v4.1 Material Resources (MR)
MRc4 Building Product Disclosure and Optimization - Material Ingredients

ASC Steel Deck Products	
1 ½” Type B Deck*	3” Type 3W Deck*	
3” Type N Deck*	7/8” Roof and Form Deck*	
2” Type 2W Deck*	4 ½”, 6”, 7 ½” Deep Deck*	
*Applies to cellular and Acustadek® (welded or riveted) version of product and offered in 18-22 gauge	

Applicable Credits:
MRc4.1 Building Product Disclosure and Optimization – Material Ingredients (1 point) or any compliant reports with third-party verification that includes the verification content inventory are worth 1.5 products for credit achievement calculations.

OPTION 1. Material Ingredients Reporting (1.5 products): ASC Steel Deck products have a third-party verified published, complete Health Product Declaration (HPD) with full disclosure of known hazards to at least 0.01% (100 parts per million) in compliance with the Health Product Declaration Open Standard v2.1.

Notable Reference:
(Option 1) This credit rewards projects who install at least 20 products from at least 5 different manufacturers that have published chemical inventories of products to at least 0.1% (1000 parts per million) using one of the approved reporting frameworks, including the HPD.
ASC Steel Deck has a third-party verified HPD with full disclosure of known hazards to at least 0.01% (100 ppm) for its portfolio of products.

ASC Steel Deck  A Division of ASC Profiles LLC 2110 Enterprise Boulevard, West Sacramento, CA 95691 Toll Free: 800.726.2727  www.ascsteeldeck.com

SCS Global Services does hereby certify that an independent assessment has been conducted on behalf of:

ASC Profiles LLC

2110 Enterprise Boulevard, West Sacramento, CA, United States

For the following product(s):
Steel Decking:
ASC Steel Deck

HPD Screening Date: 4/4/2019 Verification # qGE-2479
The product(s) meet(s) all of the necessary qualifications to be certified for the following claim(s):
Verified Health Product Declaration
This validation conforms to the Health Product Declaration Open Standard, Version 2.1.1 (Jul 2, 2018). Products have a complete, nested materials method, material threshold HPD and have been validated for health hazard warnings using full disclosure at an inventory threshold of 100 ppm (0.01%).
Registration # SCS-HPD-04790
Valid from: May 24, 2019 to April 4, 2022

Stanley Mathuram, PE, Vice President
SCS Global Services
2000 Powell Street, Ste. 600, Emeryville, CA 94608 USA

ASC Steel Deck by ASC Profiles

CLASSIFICATION:	05 31 00

Health Product Declaration v2.1.1
created via: HPDC Online Builder

PRODUCT DESCRIPTION:	ASC Steel Deck decking profiles (all) - Structural steel deck is used in roof and floor applications. Steel Deck is available in a variety of depths, widths and rib-spacings based on customer requirements. Product options include the application of a primer for field paint application ease. Product accessories include the use of insulation batts in cellular deck to improve acoustical performance.

CONTENT INVENTORY
Inventory Reporting Format Nested Materials  Method Basic Method

Threshold Disclosed Per
Material Product

Threshold level
100 ppm
1,000 ppm Per GHS SDS
Per OSHA MSDS
Other

Residuals/Impurities
Residuals/Impurities Considered in 1 of 2 Materials

Explanation(s) provided for Residuals/Impurities?
Yes	No

All Substances Above the Threshold Indicated Are:

Characterized	 Yes Ex/SC  Yes  No
% weight and role provided for all substances.

Screened	 Yes Ex/SC  Yes  No
All substances screened using Priority Hazard Lists with results disclosed.

Identified	 Yes Ex/SC  Yes  No
All substances disclosed by Name (Specific or Generic) and Identifier.

CONTENT IN DESCENDING ORDER OF QUANTITY

Summary of product contents and results from screening individual chemical substances against HPD Priority Hazard Lists and the GreenScreen for Safer Chemicals®. The HPD does not assess whether using or handling this product will expose individuals to its chemical substances or any health risk. Refer to Section 2 for further details.
MATERIAL | SUBSTANCE | RESIDUAL OR IMPURITY
GREENSCREEN SCORE | HAZARD TYPE

LT-1

LT-P

LT-UNK

BM-2

BASE STEEL [ IRON LT-P1 | END MANGANESE LT-P1 | END | MUL | REP

Number of Greenscreen BM-4/BM3 contents ... 0
Contents highest concern GreenScreen Benchmark or List translator Score ... LT-1
Nanomaterial ... No
INVENTORY AND SCREENING NOTES:

CARBON LT-UNK PHOSPHORUS
RES | PHY | END SULFUR

| PHY | MAM ALUMINUM	1 |
| SKI SILICON LT-UNK NICKEL	|

LT-P1

LT-P1

RES | CAN | SKI | MAM | MUL CHROMIUM LT-P1 | RES | END | SKI ] ZINC

METALLIC COATING [ ZINC
LT-P1 | RES | PHY | END IRON

| AQU | PHY | END | MUL ALUMINUM
| END ]

VOLATILE ORGANIC COMPOUND (VOC) CONTENT
VOC Content data is not applicable for this product category.

CERTIFICATIONS AND COMPLIANCE See Section 3 for additional listings. VOC emissions: CDPH Standard Method V1.2 (Section 1350/CHPS) - Not Applicable

CONSISTENCY WITH OTHER PROGRAMS

Pre-checked for LEED v4 Material Ingredients, Option 1

Nested Method / Material Threshold

Section 1: Summary

Third Party Verified?
Yes No

PREPARER: Self-Prepared VERIFIER: SCS Global Services VERIFICATION #: qGE-2479

SCREENING DATE: 2019-04-04
PUBLISHED DATE: 2019-05-24
EXPIRY DATE: 2022-04-04

Section 2: Content in Descending Order of Quantity

This section lists contents in a product based on specific threshold(s) and reports detailed health information including hazards. This HPD uses the inventory method indicated above, which is one of three possible methods:
Basic Inventory method with Product-level threshold.
Nested Material Inventory method with Product-level threshold
Nested Material Inventory method with individual Material-level thresholds
Definitions and requirements for the three inventory methods and requirements for each data field can be found in the HPD Open Standard version 2.1.1, available on the HPDC website at: www.hpd-collaborative.org/hpd-2-1-1-standard

BASE STEEL	%: 95.65 - 99.16

MATERIAL THRESHOLD: 100 ppm	RESIDUALS AND IMPURITIES CONSIDERED: Yes

RESIDUALS AND IMPURITIES NOTES: Residuals and impurities were considered based on direct testing conducted by steel suppliers via atomic absorption. Per best practice guidelines residuals and impurities above the reporting threshold of 100ppm with a GS score of BM-1, LT-1, LT-P1 or NoGS have been reported in the content inventory. Other residuals and impurities that might be present above the 100ppm are Copper (0.1540% max), Molybdenium (0.0500% max), Tin (0.0500% max) and Titanium (0.0100%max). Vanadium and/or Columbium may be present as residuals in steel below the inventory reporting threshold of 100ppm.

OTHER MATERIAL NOTES: The weight contribution of the base steel will vary depending on the thickness of the steel and they weight of the zinc metallic coating. See Section 5 for additional details.

IRON			ID: 7439-89-6	

HAZARD SCREENING	
METHOD:	Pharos Chemical and Materials Library	HAZARD SCREENING DATE: 2019-04-04	
%: 98.14 - 99.83

HAZARD TYPE

ENDOCRINE	GS: LT-P1

AGENCY AND LIST TITLES

TEDX - Potential Endocrine Disruptors	RC: UNK	NANO: No	ROLE: Physical Structure

WARNINGS

Potential Endocrine Disruptor	

SUBSTANCE NOTES: Percentage is a range due to variations between specified steel chemistries and grades.	

MANGANESE		ID: 7439-96-5	

HAZARD SCREENING METHOD:	Pharos Chemical and Materials Library	HAZARD SCREENING DATE: 2019-04-04	
%: 0.15 - 1.20

HAZARD TYPE

ENDOCRINE MULTIPLE

REPRODUCTIVE	GS: LT-P1

AGENCY AND LIST TITLES

TEDX - Potential Endocrine Disruptors

German FEA - Substances Hazardous to Waters

Japan - GHS	RC: UNK	NANO: No	ROLE: Physical Structure

WARNINGS

Potential Endocrine Disruptor Class 2 - Hazard to Waters

Toxic to reproduction - Category 1B	

SUBSTANCE NOTES: Percentage is a range due to variations between specified steel chemistries and grades.	

CARBON			ID: 7440-44-0	

HAZARD SCREENING	
METHOD:	Pharos Chemical and Materials Library	HAZARD SCREENING DATE: 2019-04-04	
%: 0.02 - 0.24

HAZARD TYPE

None found	GS: LT-UNK

AGENCY AND LIST TITLES	RC: UNK

WARNINGS	NANO: No	ROLE: Physical Structure

No warnings found on HPD Priority Hazard Lists	

SUBSTANCE NOTES: Percentage is a range due to variations between specified steel chemistries and grades.	

PHOSPHORUS	ID: 7723-14-0	
HAZARD SCREENING METHOD: Pharos Chemical and Materials Library	HAZARD SCREENING DATE: 2019-04-04	
%: 0.00 - 0.03	GS: BM-2	RC: UNK	NANO: No	ROLE: Physical Structure	

HAZARD TYPE	

AGENCY AND LIST TITLES	

WARNINGS	

PHYSICAL HAZARD (REACTIVE)	
EU - GHS (H-Statements)	
H228 - Flammable solid	

MAMMALIAN	
US EPA - EPCRA Extremely Hazardous	
Extremely Hazardous Substances	
	Substances		

SUBSTANCE NOTES: Percentage is a range due to variations between specified steel chemistries and grades. Priority List of Hazardous Substances (rank 19)	

ALUMINUM	ID: 7429-90-5	
HAZARD SCREENING METHOD: Pharos Chemical and Materials Library	HAZARD SCREENING DATE: 2019-04-04	
%: 0.00 - 0.10	GS: LT-P1	RC: UNK	NANO: No	ROLE: Physical Structure	

HAZARD TYPE	

AGENCY AND LIST TITLES	

WARNINGS	

RESPIRATORY	
AOEC - Asthmagens	
Asthmagen (Rs) - sensitizer-induced	

PHYSICAL HAZARD (REACTIVE)	
EU - GHS (H-Statements)	
H228 - Flammable solid	

PHYSICAL HAZARD (REACTIVE)	
EU - GHS (H-Statements)	
H250 - Catches fire spontaneously if exposed to air	

PHYSICAL HAZARD (REACTIVE)	
EU - GHS (H-Statements)	
H261 - In contact with water releases flammable gases	

ENDOCRINE	
TEDX - Potential Endocrine Disruptors	
Potential Endocrine Disruptor	

SUBSTANCE NOTES: Percentage is a range due to variations between specified steel chemistries and grades. The Priority List of Hazardous Substances (rank 179)	

SULFUR		ID: 7704-34-9	
HAZARD SCREENING METHOD: Pharos Chemical and Materials Library	HAZARD SCREENING DATE: 2019-04-04		

%: 0.00 - 0.04

GS: LT-UNK

RC: UNK

NANO: No

ROLE: Physical Structure

SUBSTANCE NOTES: Percentage is a range due to variations between specified steel chemistries and grades.

HAZARD TYPE	AGENCY AND LIST TITLES	WARNINGS	

SKIN IRRITATION	
EU - GHS (H-Statements)	
H315 - Causes skin irritation	

SILICON			ID: 7440-21-3	

HAZARD SCREENING	
METHOD:	Pharos Chemical and Materials Library	HAZARD SCREENING DATE: 2019-04-04	
%: 0.00 - 0.25

HAZARD TYPE

None found	GS: LT-UNK

AGENCY AND LIST TITLES	RC: UNK

WARNINGS	NANO: No	ROLE: Physical Structure

No warnings found on HPD Priority Hazard Lists	

SUBSTANCE NOTES: Percentage is a range due to variations between specified steel chemistries and grades.	

NICKEL		ID: 7440-02-0	

HAZARD SCREENING METHOD:	Pharos Chemical and Materials Library	HAZARD SCREENING DATE: 2019-04-04	
%: Impurity/Residual

HAZARD TYPE

RESPIRATORY CANCER CANCER CANCER CANCER CANCER CANCER
SKIN SENSITIZE CANCER
ORGAN TOXICANT

MULTIPLE

CANCER

RESPIRATORY	GS: LT-1

AGENCY AND LIST TITLES

AOEC - Asthmagens IARC
IARC

CA EPA - Prop 65

US CDC - Occupational Carcinogens US NIH - Report on Carcinogens
US NIH - Report on Carcinogens EU - GHS (H-Statements)
EU - GHS (H-Statements) EU - GHS (H-Statements)

German FEA - Substances Hazardous to Waters

MAK

MAK	RC: UNK	NANO: No	ROLE: Impurity/Residual

WARNINGS

Asthmagen (Rs) - sensitizer-induced

Group 1 - Agent is Carcinogenic to humans Group 2b - Possibly carcinogenic to humans Carcinogen
Occupational Carcinogen

Known to be a human Carcinogen

Reasonably Anticipated to be Human Carcinogen H317 - May cause an allergic skin reaction
H351 - Suspected of causing cancer

H372 - Causes damage to organs through prolonged or repeated exposure

Class 2 - Hazard to Waters

Carcinogen Group 1 - Substances that cause cancer in man

Sensitizing Substance Sah - Danger of airway & skin sensitization	

SUBSTANCE NOTES: Percentage is a range due to variations between specified steel chemistries and grades.

CHROMIUM		ID: 7440-47-3	

HAZARD SCREENING METHOD:	Pharos Chemical and Materials Library	HAZARD SCREENING DATE: 2019-04-04	
%: Impurity/Residual	GS: LT-P1	RC: UNK	NANO: No	ROLE: Impurity/Residual	

HAZARD TYPE	

AGENCY AND LIST TITLES	

WARNINGS	

RESPIRATORY	
AOEC - Asthmagens	
Asthmagen (Rs) - sensitizer-induced	

ENDOCRINE	
TEDX - Potential Endocrine Disruptors	
Potential Endocrine Disruptor	

SKIN SENSITIZE	
MAK	
Sensitizing Substance Sh - Danger of skin sensitization	

SUBSTANCE NOTES: Percentage is a range due to variations between specified steel chemistries and grades.	

ZINC METALLIC COATING	%: 0.84 - 4.35

MATERIAL THRESHOLD: 100 ppm	RESIDUALS AND IMPURITIES CONSIDERED: No

RESIDUALS AND IMPURITIES NOTES: Guidance for considering, identifying and quantifying residuals is in pilot test phase. Residuals will be considered and updated once a guideline is finalized.

OTHER MATERIAL NOTES: Zinc alloy applied by the hot dip galvanization process per the latest version of ASTM A653 Standard Specification for Steel Sheet, Zinc-Coated (Galvanized) or Zinc-Iron Alloy-Coated (Galvannealed) by the Hot- Dip Process. The weight contribution of the zinc metallic coating will vary depending on thickness of the base steel and the coating weight of zinc applied. See Section 5 for additional details.

ZINC	ID: 7440-66-6	
HAZARD SCREENING METHOD:  Pharos Chemical and Materials Library	HAZARD SCREENING DATE: 2019-04-04	
%: 99.20 - 99.50	GS: LT-P1	RC: UNK	NANO: No	ROLE: Corrosion Protection

HAZARD TYPE	AGENCY AND LIST TITLES	WARNINGS

ACUTE AQUATIC	EU - GHS (H-Statements)	H400 - Very toxic to aquatic life
CHRON AQUATIC	EU - GHS (H-Statements)	H410 - Very toxic to aquatic life with long lasting effects PHYSICAL HAZARD (REACTIVE)	EU - GHS (H-Statements)	H250 - Catches fire spontaneously if exposed to air PHYSICAL HAZARD (REACTIVE)	EU - GHS (H-Statements)	H260 - In contact with water releases flammable gases
which may ignite spontaneously

ENDOCRINE	TEDX - Potential Endocrine Disruptors	Potential Endocrine Disruptor

MULTIPLE	German FEA - Substances Hazardous to	Class 2 - Hazard to Waters Waters	

SUBSTANCE NOTES: Priority List of Hazardous Substances (rank 75).	

ALUMINUM	ID: 7429-90-5	
HAZARD SCREENING METHOD: Pharos Chemical and Materials Library	HAZARD SCREENING DATE: 2019-04-04	
%: 0.10 - 0.50	GS: LT-P1	RC: UNK	NANO: No	ROLE: Adhesion Promoter	

HAZARD TYPE	

AGENCY AND LIST TITLES	

WARNINGS	

RESPIRATORY	
AOEC - Asthmagens	
Asthmagen (Rs) - sensitizer-induced	

PHYSICAL HAZARD (REACTIVE)	
EU - GHS (H-Statements)	
H228 - Flammable solid	

PHYSICAL HAZARD (REACTIVE)	
EU - GHS (H-Statements)	
H250 - Catches fire spontaneously if exposed to air	

PHYSICAL HAZARD (REACTIVE)	
EU - GHS (H-Statements)	
H261 - In contact with water releases flammable gases	

ENDOCRINE	
TEDX - Potential Endocrine Disruptors	
Potential Endocrine Disruptor	

SUBSTANCE NOTES: Priority List of Hazardous Substances (rank 179).	

IRON			ID: 7439-89-6	

HAZARD SCREENING	
METHOD:	Pharos Chemical and Materials Library	HAZARD SCREENING DATE: 2019-04-04	
%: 0.00 - 0.02

HAZARD TYPE

ENDOCRINE	GS: LT-P1

AGENCY AND LIST TITLES

TEDX - Potential Endocrine Disruptors	RC: UNK	NANO: No

WARNINGS

Potential Endocrine Disruptor	ROLE: Metal Alloy	

SUBSTANCE NOTES: By product of the galvanization process.	

This section lists applicable certification and standards compliance information for VOC emissions and VOC content. Other types of health or environmental performance testing or certifications completed for the product may be provided.

VOC EMISSIONS	CDPH Standard Method V1.2 (Section 1350/CHPS) - Not Applicable

CERTIFYING PARTY: Self-declared APPLICABLE FACILITIES: NA CERTIFICATE URL:

ISSUE DATE: 2019-
04-04

EXPIRY DATE:	CERTIFIER OR LAB: NA

Section 3: Certifications and Compliance

CERTIFICATION AND COMPLIANCE NOTES: Not Applicable

Section 4: Accessories

This section lists related products or materials that the manufacturer requires or recommends for installation (such as adhesives or fasteners), maintenance, cleaning, or operations. For information relating to the contents of these related products, refer to their applicable Health Product Declarations, if available.

INSULATION BOARD	HPD URL: No HPD available

CONDITION WHEN RECOMMENDED OR REQUIRED AND/OR OTHER NOTES:
Insulation Board from Knauf insulation can be added to cellular flutes of structural deck at point of manufacture. This improves the acoustical properties of the installed product. Product with insulation is called 'Acustadek' or Acoustical Deck. More product information available here: https://www.pharosproject.net/material/show/2001265

DECK PRIMER	HPD URL: No HPD link provided

CONDITION WHEN RECOMMENDED OR REQUIRED AND/OR OTHER NOTES:
White or gray water-based primer available as specified by customer. When ordered with primer product is referred to as Primeshield. See Section 5 General Notes for more detail.

Section 5: General Notes

Residuals reported per chemical analysis by steel suppliers. Deck Primer is a product option but weight max in finished Steel Deck is 0.0099%. The weight contribution of steel and metallic coating to the finished product will vary based on the gauge (thickness) of the base steel and weight of the metallic coating. All figures referenced in this guide reflect 22 gauge material and a G90 coating (a combination of 95.65% steel and 4.35% metallic coating). This represents the lightest standard offer base steel and heaviest metallic coating combination. All metallic coated steel deck has a contribution ratio of steel between 96.65% -99.16% and a metallic coating range of 4.35%-0.84%. Prime shield (primer painted) or 'Cold Rolled' steel deck does not have a metallic coating and steel will represent 100% of product weight.

MANUFACTURER INFORMATION

MANUFACTURER: ASC Profiles
ADDRESS: 2110 Enterprise Blvd West Sacramento CA 95691, US WEBSITE: www.ascprofiles.com

CONTACT NAME: Michelle Vondran
TITLE: Technical Manager
PHONE: 909-484-4623
EMAIL: michelle.vondran@bluescope.us

KEY
OSHA MSDS Occupational Safety and Health Administration Material Safety Data Sheet
GHS SDS Globally Harmonized System of Classification and Labeling of Chemicals Safety Data Sheet

Hazard Types
AQU Aquatic toxicity
CAN Cancer
DEV Developmental toxicity
END Endocrine activity
EYE Eye irritation/corrosivity
GEN Gene mutation

GLO Global warming
MAM Mammalian/systemic/organ toxicity
MUL Multiple hazards NEU Neurotoxicity OZO Ozone depletion
PBT Persistent Bioaccumulative Toxic

PHY Physical Hazard (reactive) REP Reproductive toxicity RES Respiratory sensitization
SKI Skin sensitization/irritation/corrosivity
LAN Land Toxicity
NF Not found on Priority Hazard Lists

GreenScreen (GS)
BM-4 Benchmark 4 (prefer-safer chemical)
BM-3 Benchmark 3 (use but still opportunity for improvement)
BM-2 Benchmark 2 (use but search for safer substitutes)
BM-1 Benchmark 1 (avoid - chemical of high concern)
BM-U Benchmark Unspecified (insuficient data to benchmark)

LT-P1 List Translator Possible Benchmark 1
LT-1 List Translator Likely Benchmark 1
LT-UNK List Translator Benchmark Unknown (insufficient information from List Translator lists to benchmark) NoGS Unknown (no data on List Translator Lists)

Section 6: References

Recycled Types
PreC Preconsumer (Post-Industrial)
PostC Postconsumer
Both Both Preconsumer and Postconsumer Unk Inclusion of recycled content is unknown None Does not include recycled content

Other Terms Inventory Methods:
Nested Method / Material Threshold Substances listed within each material per threshold indicated per material Nested Method / Product Threshold Substances listed within each material per threshold indicated per product Basic Method / Product Threshold Substances listed individually per threshold indicated per product
Nano Composed of nano scale particles or nanotechnology
Third Party Verified Verification by independent certifier approved by HPDC Preparer Third party preparer, if not self-prepared by manufacturer Applicable facilities Manufacturing sites to which testing applies

The Health Product Declaration (HPD) Open Standard provides for the disclosure of product contents and potential associated human and environmental health hazards. Hazard associations are based on the HPD Priority Hazard Lists, the GreenScreen List Translator™, and when available, full GreenScreen® assessments. The HPD Open Standard v2.1 is not:
a method for the assessment of exposure or risk associated with product handling or use,
a method for assessing potential health impacts of: (i) substances used or created during the manufacturing process or (ii) substances created after the product is delivered for end use.
Information about life cycle, exposure and/or risk assessments performed on the product may be reported by the manufacturer in appropriate Notes sections, and/or, where applicable, in the Certifications section.
The HPD Open Standard was created and is supported by the Health Product Declaration Collaborative (the HPD Collaborative), a customer-led organization composed of stakeholders throughout the building industry that is committed to the continuous improvement of building products through transparency, openness, and innovation throughout the product supply chain.
The product manufacturer and any applicable independent verifier are solely responsible for the accuracy of statements and claims made in this HPD and for compliance with the HPD standard noted.