Smooth Series Cellular Deck.
Rivets flush with exposed surface.
Clean beam-pan rivet attachment.
No more unsightly burn mark!
Rivet attachments uniformly repeated along deck profile.
Rivets match factory applied primer.
No field touch-up required!
Learn more at www.ascsd.com
ASC Steel Deck